**441/2**

**HOMESCIENCE**

**(CLOTHING CONSTRUCTION)**

**(PRACTICAL)**

**PAPER 2**

**2 ½ HOURS**

**FORM 4**

**Kenya certificate of secondary education (K.C.S.E)**

**HOMESCIENCE (CLOTHING CONSTRUCTION)**

**PAPER 2**

**(PRACTICAL)**

**2 ½ HOURS**

***This paper consists of 2 printed pages. Candidates should check the question paper to ensure that all pages are printed as indicated and no questions are missing.***

A pattern of girl’s bodice is provided. You are advised to study the sketches, instructions and the layout carefully before you begin the test.

**MATERIALS PROVIDED**

1.Pattern pieces.

A- Front bodice.

B- Back bodice.

C- Sleeve.

D- Collar.

E- Back neck facing.

2. Plain light weight fabric 54cm long by 90cm wide.

3. Sewing thread to match the fabric.

**THE TEST**

Using the materials provided, cut out and make the front bodice to show the following:

1. The making of a shoulder dart on the back bodice.
2. The making of the shoulder seam using a machine fell seam:
3. Joining of the front and back neck facings at the shoulder.
4. Neatening of the free edge of the joined facing.
5. The preparation of the interfaced collar.
6. Attaching of the collar using the joined facings.
7. The working of the side seam using a french seam.
8. The darning of the hedge tear on the sleeve. (Make a tear as shown on the pattern piece)
9. Preparation of sleeve to include:
10. Gathering of the sleeve crown.
11. Working of the sleeve seam using a neatened plain seam.
12. Working of a machined hem on the lower edge of the sleeve.

At the end of the examination, firmly sew onto your work, on a single fabric, a label bearing your name and index number. Remove the needle and pins from your work, then fold your work neatly and place it in the envelope provided. Do not put scraps of fabric in the envelope.